<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="50" x2="0" y2="5" width="0" layer="20"/>
<wire x1="0" y1="5" x2="5" y2="0" width="0" layer="20" curve="90"/>
<wire x1="5" y1="0" x2="55" y2="0" width="0" layer="20"/>
<wire x1="55" y1="0" x2="60" y2="5" width="0" layer="20" curve="90"/>
<wire x1="60" y1="5" x2="60" y2="50" width="0" layer="20"/>
<wire x1="60" y1="50" x2="55" y2="55" width="0" layer="20" curve="90"/>
<wire x1="55" y1="55" x2="5" y2="55" width="0" layer="20"/>
<wire x1="5" y1="55" x2="0" y2="50" width="0" layer="20" curve="90"/>
<text>025</text>
<text>MMXXIII</text>
<text>470 MHz Low Pass Filter</text>
<text>IN</text>
<text>OUT</text>
<text>THROUGH CAL</text>
</plain>
<libraries>
<library name="ruark2">
<packages>
<package name="0603">
</package>
<package name="CONREVSMA008-G">
</package>
<package name="2118714-2">
</package>
<package name="GA3092">
</package>
<package name="2222SQ-111">
</package>
<package name="JZ300">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="ruark2" package="0603" value="2.2pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="ruark2" package="0603" value="2.2pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="ruark2" package="0603" value="2.2pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="ruark2" package="0603" value="2.2pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="ruark2" package="0603" value="1.3pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="ruark2" package="CONREVSMA008-G" value="0733910070">
<attribute name="NAME"/>
<attribute name="PARTNO" value="WM5544-ND"/>
</element>
<element name="J2" library="ruark2" package="CONREVSMA008-G" value="0733910070">
<attribute name="NAME"/>
<attribute name="PARTNO" value="WM5544-ND"/>
</element>
<element name="SH1" library="ruark2" package="2118714-2" value="2118714-2">
<attribute name="NAME"/>
<attribute name="PARTNO" value="A126151CT-ND"/>
</element>
<element name="SH2" library="ruark2" package="2118714-2" value="2118714-2">
<attribute name="NAME"/>
<attribute name="PARTNO" value="A126151CT-ND"/>
</element>
<element name="J3" library="ruark2" package="CONREVSMA008-G" value="0733910070">
<attribute name="NAME"/>
<attribute name="PARTNO" value="WM5544-ND"/>
</element>
<element name="J4" library="ruark2" package="CONREVSMA008-G" value="0733910070">
<attribute name="NAME"/>
<attribute name="PARTNO" value="WM5544-ND"/>
</element>
<element name="J5" library="ruark2" package="CONREVSMA008-G" value="0733910070">
<attribute name="NAME"/>
<attribute name="PARTNO" value="WM5544-ND"/>
</element>
<element name="J6" library="ruark2" package="CONREVSMA008-G" value="0733910070">
<attribute name="NAME"/>
<attribute name="PARTNO" value="WM5544-ND"/>
</element>
<element name="L4" library="ruark2" package="GA3092" value="3.7nH">
<attribute name="NAME"/>
</element>
<element name="L5" library="ruark2" package="2222SQ-111" value="110nH">
<attribute name="NAME"/>
</element>
<element name="C5" library="ruark2" package="JZ300" value="1.5-3pF">
<attribute name="NAME"/>
<attribute name="PARTNO" value=""/>
</element>
<element name="C6" library="ruark2" package="0603" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="L4" pad="P$1"/>
<contactref element="C5" pad="HOT"/>
<contactref element="C8" pad="2"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="J1" pad="G1"/>
<contactref element="J1" pad="G2"/>
<contactref element="J1" pad="G3"/>
<contactref element="J1" pad="G4"/>
<contactref element="J2" pad="G1"/>
<contactref element="J2" pad="G2"/>
<contactref element="J2" pad="G3"/>
<contactref element="J2" pad="G4"/>
<contactref element="J3" pad="G1"/>
<contactref element="J3" pad="G3"/>
<contactref element="J3" pad="G4"/>
<contactref element="J3" pad="G2"/>
<contactref element="J4" pad="G1"/>
<contactref element="J4" pad="G3"/>
<contactref element="J4" pad="G4"/>
<contactref element="J4" pad="G2"/>
<contactref element="SH1" pad="P$12"/>
<contactref element="SH1" pad="P$2"/>
<contactref element="SH1" pad="P$7"/>
<contactref element="SH1" pad="P$11"/>
<contactref element="SH1" pad="P$6"/>
<contactref element="SH1" pad="P$10"/>
<contactref element="SH1" pad="P$1"/>
<contactref element="SH1" pad="P$9"/>
<contactref element="SH1" pad="P$5"/>
<contactref element="SH1" pad="P$8"/>
<contactref element="SH1" pad="P$4"/>
<contactref element="SH1" pad="P$3"/>
<contactref element="SH2" pad="P$12"/>
<contactref element="SH2" pad="P$2"/>
<contactref element="SH2" pad="P$7"/>
<contactref element="SH2" pad="P$11"/>
<contactref element="SH2" pad="P$6"/>
<contactref element="SH2" pad="P$10"/>
<contactref element="SH2" pad="P$1"/>
<contactref element="SH2" pad="P$9"/>
<contactref element="SH2" pad="P$5"/>
<contactref element="SH2" pad="P$8"/>
<contactref element="SH2" pad="P$4"/>
<contactref element="SH2" pad="P$3"/>
<contactref element="J5" pad="G2"/>
<contactref element="J5" pad="G3"/>
<contactref element="J5" pad="G4"/>
<contactref element="J5" pad="G1"/>
<contactref element="J6" pad="G2"/>
<contactref element="J6" pad="G3"/>
<contactref element="J6" pad="G4"/>
<contactref element="J6" pad="G1"/>
<contactref element="C5" pad="COLD"/>
<contactref element="L4" pad="P$2"/>
</signal>
<signal name="N$7">
<contactref element="J4" pad="S"/>
<contactref element="J3" pad="S"/>
</signal>
<signal name="N$5">
<contactref element="J6" pad="S"/>
<contactref element="J5" pad="S"/>
</signal>
<signal name="N$2">
<contactref element="C8" pad="1"/>
<contactref element="L5" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="L5" pad="P$2"/>
<contactref element="J2" pad="S"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="S"/>
<contactref element="C6" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
