<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<schematic>
<libraries>
<library name="ruark2">
<packages>
<package name="2118714-2">
</package>
<package name="111SQ-36N">
</package>
<package name="1111SQ-47N">
</package>
<package name="CONREVSMA008-G">
</package>
<package name="0603">
</package>
</packages>
<symbols>
<symbol name="SHIELD">
<pin name="P$1"/>
</symbol>
<symbol name="INDUCTOR">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="COAX">
<pin name="RF"/>
<pin name="GND"/>
</symbol>
<symbol name="C">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="2118714-2" prefix="SH">
<description>RF Shield Frame 0.500" (12.70mm) X 0.538" (13.66mm) Surface Mount</description>
<gates>
<gate name="G$1" symbol="SHIELD"/>
</gates>
<devices>
<device name="" package="2118714-2">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1 P$2 P$3 P$4 P$5 P$6 P$7 P$8 P$9 P$10 P$11 P$12"/>
</connects>
<technologies>
<technology name="">
<attribute name="PARTNO" value="A126151CT-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1111SQ-36NGEC" prefix="L">
<description>RF Inductors - SMD 1111 36nH Unshld 2% 4.8A 9.8mOhms</description>
<gates>
<gate name="G$1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="" package="111SQ-36N">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="VALUE" value="36nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1111SQ-47N" prefix="L">
<description>RF Inductors - SMD 1111 47nH Unshld 2% 4.4A 11.3mOhms</description>
<gates>
<gate name="G$1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="" package="1111SQ-47N">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="VALUE" value="47nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="0733910070" prefix="J">
<description>SMA Connector Receptacle, Female Socket 50Ohm Through Hole Solder</description>
<gates>
<gate name="G$1" symbol="COAX"/>
</gates>
<devices>
<device name="" package="CONREVSMA008-G">
<connects>
<connect gate="G$1" pin="GND" pad="G1 G2 G3 G4"/>
<connect gate="G$1" pin="RF" pad="S"/>
</connects>
<technologies>
<technology name="">
<attribute name="PARTNO" value="WM5544-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="0603_CAPACITOR" prefix="C">
<description>0603 Capacitor -- WARNING: NO DEFINED VALUE OR PART NUMBER</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="VALUE" value="sel"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply1">
<description>&lt;b&gt;Supply Symbols&lt;/b&gt;&lt;p&gt;
 GND, VCC, 0V, +5V, -5V, etc.&lt;p&gt;
 Please keep in mind, that these devices are necessary for the
 automatic wiring of the supply signals.&lt;p&gt;
 The pin name defined in the symbol is identical to the net which is to be wired automatically.&lt;p&gt;
 In this library the device names are the same as the pin names of the symbols, therefore the correct signal names appear next to the supply symbols in the schematic.&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
</packages>
<symbols>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="SH1" library="ruark2" deviceset="2118714-2" device=""/>
<part name="SH2" library="ruark2" deviceset="2118714-2" device=""/>
<part name="L1" library="ruark2" deviceset="1111SQ-36NGEC" device="" value="36nH"/>
<part name="L2" library="ruark2" deviceset="1111SQ-47N" device="" value="47nH"/>
<part name="J1" library="ruark2" deviceset="0733910070" device=""/>
<part name="J2" library="ruark2" deviceset="0733910070" device=""/>
<part name="C1" library="ruark2" deviceset="0603_CAPACITOR" device="" value="2.2pF"/>
<part name="C2" library="ruark2" deviceset="0603_CAPACITOR" device="" value="2.2pF"/>
<part name="C3" library="ruark2" deviceset="0603_CAPACITOR" device="" value="2.2pF"/>
<part name="C4" library="ruark2" deviceset="0603_CAPACITOR" device="" value="2.2pF"/>
<part name="C5" library="ruark2" deviceset="0603_CAPACITOR" device="" value="2.2pF"/>
<part name="C6" library="ruark2" deviceset="0603_CAPACITOR" device="" value="2.2pF"/>
<part name="C7" library="ruark2" deviceset="0603_CAPACITOR" device="" value="2.2pF"/>
<part name="C8" library="ruark2" deviceset="0603_CAPACITOR" device="" value="2.2pF"/>
<part name="L3" library="ruark2" deviceset="1111SQ-36NGEC" device="" value="36nH"/>
<part name="GND1" library="supply1" deviceset="GND" device=""/>
<part name="GND2" library="supply1" deviceset="GND" device=""/>
<part name="GND3" library="supply1" deviceset="GND" device=""/>
<part name="GND4" library="supply1" deviceset="GND" device=""/>
<part name="GND5" library="supply1" deviceset="GND" device=""/>
<part name="GND6" library="supply1" deviceset="GND" device=""/>
<part name="GND7" library="supply1" deviceset="GND" device=""/>
<part name="GND8" library="supply1" deviceset="GND" device=""/>
<part name="C9" library="ruark2" deviceset="0603_CAPACITOR" device="" value="1pF"/>
<part name="C10" library="ruark2" deviceset="0603_CAPACITOR" device="" value="1pF"/>
<part name="GND9" library="supply1" deviceset="GND" device=""/>
<part name="GND10" library="supply1" deviceset="GND" device=""/>
<part name="GND11" library="supply1" deviceset="GND" device=""/>
<part name="GND12" library="supply1" deviceset="GND" device=""/>
<part name="J3" library="ruark2" deviceset="0733910070" device=""/>
<part name="GND13" library="supply1" deviceset="GND" device=""/>
<part name="J4" library="ruark2" deviceset="0733910070" device=""/>
<part name="GND14" library="supply1" deviceset="GND" device=""/>
<part name="GND15" library="supply1" deviceset="GND" device=""/>
<part name="GND16" library="supply1" deviceset="GND" device=""/>
</parts>
<sheets>
<sheet>
<plain>
<text>Target 8.2pF</text>
<text>Target 8.2pF</text>
</plain>
<busses>
</busses>
<nets>
<net name="N$1">
<segment>
<pinref part="L1" gate="G$1" pin="P$2"/>
<pinref part="L2" gate="G$1" pin="P$1"/>
<pinref part="C1" gate="G$1" pin="1"/>
<pinref part="C2" gate="G$1" pin="1"/>
<pinref part="C3" gate="G$1" pin="1"/>
<pinref part="C4" gate="G$1" pin="1"/>
</segment>
</net>
<net name="GND">
<segment>
<pinref part="GND1" gate="1" pin="GND"/>
<pinref part="C1" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND2" gate="1" pin="GND"/>
<pinref part="C2" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND3" gate="1" pin="GND"/>
<pinref part="C3" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND4" gate="1" pin="GND"/>
<pinref part="C4" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND5" gate="1" pin="GND"/>
<pinref part="C5" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND6" gate="1" pin="GND"/>
<pinref part="C6" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND7" gate="1" pin="GND"/>
<pinref part="C7" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND8" gate="1" pin="GND"/>
<pinref part="C8" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND9" gate="1" pin="GND"/>
<pinref part="C9" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND10" gate="1" pin="GND"/>
<pinref part="J1" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="GND12" gate="1" pin="GND"/>
<pinref part="J2" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="GND11" gate="1" pin="GND"/>
<pinref part="C10" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND13" gate="1" pin="GND"/>
<pinref part="J3" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="GND14" gate="1" pin="GND"/>
<pinref part="J4" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="SH1" gate="G$1" pin="P$1"/>
<pinref part="GND15" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="SH2" gate="G$1" pin="P$1"/>
<pinref part="GND16" gate="1" pin="GND"/>
</segment>
</net>
<net name="N$2">
<segment>
<pinref part="L2" gate="G$1" pin="P$2"/>
<pinref part="L3" gate="G$1" pin="P$1"/>
<pinref part="C8" gate="G$1" pin="1"/>
<pinref part="C7" gate="G$1" pin="1"/>
<pinref part="C6" gate="G$1" pin="1"/>
<pinref part="C5" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$3">
<segment>
<pinref part="L1" gate="G$1" pin="P$1"/>
<pinref part="J1" gate="G$1" pin="RF"/>
<pinref part="C9" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$4">
<segment>
<pinref part="L3" gate="G$1" pin="P$2"/>
<pinref part="J2" gate="G$1" pin="RF"/>
<pinref part="C10" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$7">
<segment>
<pinref part="J4" gate="G$1" pin="RF"/>
<pinref part="J3" gate="G$1" pin="RF"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
